,_distributed by##OTHER##,_current revision##OTHER##,_created by##OTHER##,_authorized by##OTHER##,_BIMspec_GUID##OTHER##,Width##LENGTH##MILLIMETERS,Waste Connection##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabor##OTHER##,WarrantyDescription##OTHER##,Void Height Offset##LENGTH##MILLIMETERS,Void Depth Offset##LENGTH##MILLIMETERS,Vent Connection##OTHER##,URL##OTHER##,TypeName##OTHER##,Type Version##OTHER##,Type Comments##OTHER##,Top Entry Inlets##OTHER##,TagNumber##OTHER##,Sustainability##OTHER##,Standards and Approvals##OTHER##,Specification Clause##OTHER##,SpareParts##OTHER##,Size##OTHER##,Show Pipe Cover##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,ReplacementCost##OTHER##,ReferencedStandard##OTHER##,Rear Entry Inlets##OTHER##,Quick Code##OTHER##,ProductionYear##OTHER##,PipeConnectionOffset##LENGTH##MILLIMETERS,Pipe Cover Warning##OTHER##,Panel & Pipe Cover Material##OTHER##,Operating Conditions##OTHER##,NBSReference##OTHER##,NBSObjectName##OTHER##,NBSNote##OTHER##,NBSDescription##OTHER##,ModelNumber##OTHER##,Mechanical Specification##OTHER##,Maximum Static Pressure##OTHER##,Material##OTHER##,Maintained Water Pressure##OTHER##,Integral Flow Rate##OTHER##,InstallationDate##OTHER##,ILTDU##OTHER##,Hot Water Radius##LENGTH##MILLIMETERS,Height To Ceiling##LENGTH##MILLIMETERS,Model##OTHER##,Manufacturer##OTHER##,Length of Head Pipe##LENGTH##MILLIMETERS,Length##LENGTH##MILLIMETERS,Keynote##OTHER##,Hot Water Connection Diameter##LENGTH##MILLIMETERS,Has Standard Controls##OTHER##,Has Pipe Cover##OTHER##,Has Key - 6263##OTHER##,Has BS 8300 Compliant Lever Controls##OTHER##,Has 940mm Pipe Cover Kit##OTHER##,Has 465mm Pipe Cover Kit##OTHER##,HW Connection Size##LENGTH##MILLIMETERS,HW Connection##OTHER##,Grade##OTHER##,Finish##OTHER##,Features##OTHER##,ExpectedLife##OTHER##,DurationUnit##OTHER##,DocumentationTechnical##OTHER##,DocumentationLiterature##OTHER##,DocumentationInstallationGuide##OTHER##,DocumentationCertificates##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Cut Length of Pipe Cover Kit##LENGTH##MILLIMETERS,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Connectors Offset##LENGTH##MILLIMETERS,Connector Z Offset##LENGTH##MILLIMETERS,Connector Y Offset##LENGTH##MILLIMETERS,Color##OTHER##,Cold Water Radius##LENGTH##MILLIMETERS,Cold Water Connection Diameter##LENGTH##MILLIMETERS,CodePerformance##OTHER##,ClassificationValue##OTHER##,ClassificationName##OTHER##,CW Connection Size##LENGTH##MILLIMETERS,CW Connection##OTHER##,BarCode##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Assembly Code##OTHER##,Applications##OTHER##,Accessories##OTHER##,AccessibilityPerformance##OTHER##,A##LENGTH##MILLIMETERS
T106A,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T106A,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH DUAL CONTROL THERMOSTATIC SHOWER VALVE AND SWIVEL SHOWER HEAD
TSV1-A106A

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and easy clean swivel shower head with flow regulator in chromium plated finish. Product Reference TSV1-A106A as per drawing No. D10339. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T106A,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T106A,"Connection to hot / cold water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in DZR brass to BSEN12165 CW602N , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable. Includes low level integral isolating valves.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A106A/,Horne TSV1 Shower panel with dual control thermostatic shower valve and swivel shower head.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineerign Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit., n/a,280.000000000000
T106B,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,2,T106B,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH DUAL CONTROL THERMOSTATIC SHOWER VALVE AND SWIVEL SHOWER HEAD
TSV1-A106AB

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and easy clean swivel shower head with flow regulator in chromium plated finish. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A106AB as per drawing D10343. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T106B,2016,0.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T106B,"Connection to hot / cold water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in DZR brass to BSEN12165 CW602N , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable. Includes low level integral isolating valves.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A106AB/,Horne TSV1 Shower panel with dual control thermostatic shower valve and swivel shower head.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineerign Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit., n/a,280.000000000000
T106A2L,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,3,T106A2L,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH DUAL CONTROL THERMOSTATIC SHOWER VALVE, LEVER CONTROLS AND SWIVEL HEAD
TSV1-A106A2L

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with BS 8300 compliant lever controls and easy clean swivel shower head with flow regulator in chromium plated finish. Product Reference TSV1-A106A2L as per drawing No. D10372. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T106A2L,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T106A2L,"Connection to hot / cold water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in DZR brass to BSEN12165 CW602N , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable. Includes low level integral isolating valves.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,0,0,1,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A106A2L/,"Horne TSV1 Shower panel with dual control thermostatic shower valve, lever controls and swivel shower head.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineerign Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,BS8300 Compliant lever controls,280.000000000000
T106B2L,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,4,T106B2L,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH DUAL CONTROL THERMOSTATIC SHOWER VALVE, LEVER CONTROLS AND SWIVEL SHOWER HEAD
TSV1-A106AB2L

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester coated aluminium panel with BS 8300 compliant lever controls and easy clean swivel shower head with flow regulator in chromium plated finish. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A106AB2L as per drawing No. D10373. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T106B2L,2016,0.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T106B2L,"Connection to hot / cold water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in DZR brass to BSEN12165 CW602N , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable. Includes low level integral isolating valves.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,0,0,1,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A106AB2L/,"Horne TSV1 Shower panel with dual control thermostatic shower valve, lever controls and swivel shower head.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineerign Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,BS8300 Compliant lever controls,280.000000000000
T106T4,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T106T4,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH DUAL CONTROL THERMOSTATIC SHOWER VALVE AND SWIVEL SHOWER HEAD
TSV1-A106A

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and easy clean swivel shower head with flow regulator in chromium plated finish. Product Reference TSV1-A106A as per drawing No. D10339. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T106T4,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T106T4,"Connection to hot / cold water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in DZR brass to BSEN12165 CW602N , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable. Includes low level integral isolating valves.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,480.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,0,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A106A/,Horne TSV1 Shower panel with dual control thermostatic shower valve and swivel shower head.,1350.000000000000,465.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineerign Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit., n/a,280.000000000000
T106T9,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T106T9,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH DUAL CONTROL THERMOSTATIC SHOWER VALVE AND SWIVEL SHOWER HEAD
TSV1-A106A

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and easy clean swivel shower head with flow regulator in chromium plated finish. Product Reference TSV1-A106A as per drawing No. D10339. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T106T9,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T106T9,"Connection to hot / cold water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in DZR brass to BSEN12165 CW602N , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable. Includes low level integral isolating valves.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,0,1,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A106A/,Horne TSV1 Shower panel with dual control thermostatic shower valve and swivel shower head.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineerign Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit., n/a,280.000000000000
