,_distributed by##OTHER##,_current revision##OTHER##,_created by##OTHER##,_authorized by##OTHER##,_BIMspec_GUID##OTHER##,Width##LENGTH##MILLIMETERS,Waste Connection##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabor##OTHER##,WarrantyDescription##OTHER##,Void Height Offset##LENGTH##MILLIMETERS,Void Depth Offset##LENGTH##MILLIMETERS,Vent Connection##OTHER##,URL##OTHER##,TypeName##OTHER##,Type Version##OTHER##,Type Comments##OTHER##,Top Entry Inlets##OTHER##,TagNumber##OTHER##,Sustainability##OTHER##,Standards and Approvals##OTHER##,Specification Clause##OTHER##,SpareParts##OTHER##,Size##OTHER##,Show Pipe Cover##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,ReplacementCost##OTHER##,ReferencedStandard##OTHER##,Rear Entry Inlets##OTHER##,Quick Code##OTHER##,ProductionYear##OTHER##,PipeConnectionOffset##LENGTH##MILLIMETERS,Pipe Cover Warning##OTHER##,Panel & Pipe Cover Material##OTHER##,Operating Conditions##OTHER##,NBSReference##OTHER##,NBSObjectName##OTHER##,NBSNote##OTHER##,NBSDescription##OTHER##,ModelNumber##OTHER##,Mechanical Specification##OTHER##,Maximum Static Pressure##OTHER##,Material##OTHER##,Maintained Water Pressure##OTHER##,Integral Flow Rate##OTHER##,InstallationDate##OTHER##,ILTDU##OTHER##,Hot Water Radius##LENGTH##MILLIMETERS,Height To Ceiling##LENGTH##MILLIMETERS,Model##OTHER##,Manufacturer##OTHER##,Length of Head Pipe##LENGTH##MILLIMETERS,Length##LENGTH##MILLIMETERS,Keynote##OTHER##,Hot Water Connection Diameter##LENGTH##MILLIMETERS,Has Standard Controls##OTHER##,Has Single Function Handset##OTHER##,Has Pipe Cover##OTHER##,Has Key - 6263##OTHER##,Has BS 8300 Compliant Lever Controls##OTHER##,Has 940mm Pipe Cover Kit##OTHER##,Has 465mm Pipe Cover Kit##OTHER##,Has 3 Function Handset##OTHER##,HW Connection Size##LENGTH##MILLIMETERS,HW Connection##OTHER##,Grade##OTHER##,Finish##OTHER##,Features##OTHER##,ExpectedLife##OTHER##,DurationUnit##OTHER##,DocumentationTechnical##OTHER##,DocumentationLiterature##OTHER##,DocumentationInstallationGuide##OTHER##,DocumentationCertificates##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Cut Length of Pipe Cover Kit##LENGTH##MILLIMETERS,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Connectors Offset##LENGTH##MILLIMETERS,Connector Z Offset##LENGTH##MILLIMETERS,Connector Y Offset##LENGTH##MILLIMETERS,Color##OTHER##,Cold Water Radius##LENGTH##MILLIMETERS,Cold Water Connection Diameter##LENGTH##MILLIMETERS,CodePerformance##OTHER##,ClassificationValue##OTHER##,ClassificationName##OTHER##,CW Connection Size##LENGTH##MILLIMETERS,CW Connection##OTHER##,BarCode##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Assembly Code##OTHER##,Applications##OTHER##,Accessories##OTHER##,AccessibilityPerformance##OTHER##,A##LENGTH##MILLIMETERS
T108B2L,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,8,T108B2L,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH LEVER CONTROLS, FLEXIBLE HOSE & SLIDE BAR AND SINGLE FUNCTION SHOWER HEAD
TSV1-A108AB2L

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with BS 8300 compliant lever controls and shower kit, comprising flow regulated chromium plated single function shower hand set with flexible hose and slide bar. Connections by SOFT-PEX flexile braided hose for concealed water supply. Product Reference TSV1-A108AB2L as per drawing No. D10369. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T108B2L,2016,88.999999999997,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T108B2L,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,0,0,1,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A108AB2L/,"Horne TSV1 Shower panel with lever controls, flexible hose and slide bar and single function hand set. Supplies from behind.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",BS8300 Compliant lever controls,280.000000000000
T108B,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,6,T108B,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH FLEXIBLE HOSE & SLIDE BAR AND SINGLE FUNCTION SHOWER HEAD
TSV1-A108AB

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and shower kit, comprising flow regulated chromium plated single function shower hand set with flexible hose and slide bar. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A108AB as per drawing D10341. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T108B,2016,88.999999999997,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T108B,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A108AB/,Horne TSV1 Shower panel with flexible hose and slide bar and single function hand set. Supplies from behind.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T108A2L,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,7,T108A2L,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH LEVER CONTROLS, FLEXIBLE HOSE & SLIDE BAR AND SINGLE FUNCTION SHOWER HEAD
TSV1-A108A2L

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with BS 8300 compliant lever controls and shower kit, comprising flow regulated chromium plated single function shower hand set with flexible hose and slide bar. Product Reference TSV1-A108A2L as per drawing No. D10367. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T108A2L,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T108A2L,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,0,0,1,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A108A2L/,"Horne TSV1 Shower panel with lever controls, flexible hose and slide bar and single function hand set. Supplies from above.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",BS8300 Compliant lever controls,280.000000000000
T108A,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,5,T108A,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH FLEXIBLE HOSE & SLIDE BAR AND SINGLE FUNCTION SHOWER HEAD
TSV1-A108A

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and shower kit, comprising flow regulated chromium plated single function shower hand set with flexible hose and slide bar. Product Reference TSV1-A108A as per drawing No. D10329. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T108A,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T108A,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A108A/,Horne TSV1 Shower panel with flexible hose and slide bar and single function hand set. Supplies from above.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T107B2L,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,4,T107B2L,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH FLEXIBLE HOSE AND SLIDE BAR AND 3 FUNCTION HAND SET
TSV1-A107AB2L

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with BS 8300 compliant lever controls and shower kit, comprising flow regulated chromium plated three function shower hand set with flexible hose and slide bar. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A107AB2L as per drawing No. D10371. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T107B2L,2016,88.999999999997,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T107B2L,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,0,0,0,1,0,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A107AB2L/,"Horne TSV1 Shower panel with lever controls, flexible hose and slide bar and 3 function hand set. Supplies from behind.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",BS8300 Compliant lever controls,280.000000000000
T107A2L,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,3,T107A2L,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH LEVER CONTROLS, FLEXIBLE HOSE AND SLIDE BAR AND 3 FUNCTION HAND SET
TSV1-A107A2L

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with BS 8300 compliant lever controls and shower kit, comprising flow regulated chromium plated three function shower hand set with flexible hose and slide bar. Product Reference TSV1-A107A2L as per drawing No. D10370. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T107A2L,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T107A2L,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,0,0,0,1,0,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A107A2L/,"Horne TSV1 Shower panel with lever controls, flexible hose and slide bar and 3 function hand set. Supplies from above.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",BS8300 Compliant lever controls,280.000000000000
T107B,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,2,T107B,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH FLEXIBLE HOSE AND SLIDE BAR AND 3 FUNCTION HAND SET
TSV1-A107AB

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and shower kit, comprising flow regulated chromium plated three function easy clean shower hand set with flexible hose and slide bar. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A107AB as per drawing D10344. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T107B,2016,88.999999999997,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T107B,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,0,0,0,0,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A107AB/,Horne TSV1 Shower panel with flexible hose and slide bar and 3 function hand set. Supplies from behind.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T107A,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T107A,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH FLEXIBLE HOSE AND SLIDE BAR AND 3 FUNCTION HAND SET
TSV1-A107A

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and shower kit, comprising flow regulated chromium plated three function easy clean shower hand set with flexible hose and slide bar. Product Reference TSV1-A107A as per drawing No. D10330. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T107A,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T107A,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,0,0,0,0,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A107A/,Horne TSV1 Shower panel with flexible hose and slide bar and 3 function hand set. Supplies from above.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T107T4,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T107T4,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH FLEXIBLE HOSE AND SLIDE BAR AND 3 FUNCTION HAND SET
TSV1-A107A

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and shower kit, comprising flow regulated chromium plated three function easy clean shower hand set with flexible hose and slide bar. Product Reference TSV1-A107A as per drawing No. D10330. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T107T4,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T107T4,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,480.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,1,0,0,0,1,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A107A/,Horne TSV1 Shower panel with flexible hose and slide bar and 3 function hand set. Supplies from above.,1350.000000000000,465.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T107T9,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T107T9,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH FLEXIBLE HOSE AND SLIDE BAR AND 3 FUNCTION HAND SET
TSV1-A107A

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and shower kit, comprising flow regulated chromium plated three function easy clean shower hand set with flexible hose and slide bar. Product Reference TSV1-A107A as per drawing No. D10330. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T107T9,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T107T9,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,1,0,0,1,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A107A/,Horne TSV1 Shower panel with flexible hose and slide bar and 3 function hand set. Supplies from above.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T108T4,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,5,T108T4,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH FLEXIBLE HOSE & SLIDE BAR AND SINGLE FUNCTION SHOWER HEAD
TSV1-A108A

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and shower kit, comprising flow regulated chromium plated single function shower hand set with flexible hose and slide bar. Product Reference TSV1-A108A as per drawing No. D10329. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T108T4,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T108T4,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,480.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,1,0,0,0,1,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A108A/,Horne TSV1 Shower panel with flexible hose and slide bar and single function hand set. Supplies from above.,1350.000000000000,465.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T108T9,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,5,T108T9,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE TSV1 SHOWER PANEL WITH FLEXIBLE HOSE & SLIDE BAR AND SINGLE FUNCTION SHOWER HEAD
TSV1-A108A

Includes integral TSV1-3 thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with hand controls and shower kit, comprising flow regulated chromium plated single function shower hand set with flexible hose and slide bar. Product Reference TSV1-A108A as per drawing No. D10329. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T108T9,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.2 - 5 bar, range of hot water supply temperatures  52 - 85 deg C, min differnetial between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T108T9,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,1,0,0,1,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Horne-Dual-Control-Shower-Valve-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-DUAL-CONTROL-THERMOSTATIC-SHOWER-VALVE-AND-SWIVEL-SHOWER-HEAD/TSV1-A108A/,Horne TSV1 Shower panel with flexible hose and slide bar and single function hand set. Supplies from above.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in secure and institutional settings.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
