,_distributed by##OTHER##,_current revision##OTHER##,_created by##OTHER##,_authorized by##OTHER##,_BIMspec_GUID##OTHER##,Width##LENGTH##MILLIMETERS,Waste Connection##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabor##OTHER##,WarrantyDescription##OTHER##,Void Height Offset##LENGTH##MILLIMETERS,Void Depth Offset##LENGTH##MILLIMETERS,Vent Connection##OTHER##,URL##OTHER##,TypeName##OTHER##,Type Version##OTHER##,Type Comments##OTHER##,Top Entry Inlets##OTHER##,TagNumber##OTHER##,Sustainability##OTHER##,Standards and Approvals##OTHER##,Specification Clause##OTHER##,SpareParts##OTHER##,Size##OTHER##,Show Pipe Cover##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,ReplacementCost##OTHER##,ReferencedStandard##OTHER##,Rear Entry Inlets##OTHER##,Quick Code##OTHER##,ProductionYear##OTHER##,PipeConnectionOffset##LENGTH##MILLIMETERS,Pipe Cover Warning##OTHER##,Panel & Pipe Cover Material##OTHER##,Operating Conditions##OTHER##,NBSReference##OTHER##,NBSObjectName##OTHER##,NBSNote##OTHER##,NBSDescription##OTHER##,ModelNumber##OTHER##,Mechanical Specification##OTHER##,Maximum Static Pressure##OTHER##,Material##OTHER##,Maintained Water Pressure##OTHER##,Integral Flow Rate##OTHER##,InstallationDate##OTHER##,ILTDU##OTHER##,Hot Water Radius##LENGTH##MILLIMETERS,Height To Ceiling##LENGTH##MILLIMETERS,Model##OTHER##,Manufacturer##OTHER##,Length of Head Pipe##LENGTH##MILLIMETERS,Length##LENGTH##MILLIMETERS,Keynote##OTHER##,Hot Water Connection Diameter##LENGTH##MILLIMETERS,Has Vandal Resistant Shower Head##OTHER##,Has Temperature Control##OTHER##,Has Swivel Shower Head##OTHER##,Has Standard Timed Flow Control##OTHER##,Has Pipe Cover##OTHER##,Has Ligature Resistant Timed Flow Control##OTHER##,Has Key - 6263##OTHER##,Has 940mm Pipe Cover Kit##OTHER##,Has 465mm Pipe Cover Kit##OTHER##,HW Connection Size##LENGTH##MILLIMETERS,HW Connection##OTHER##,Grade##OTHER##,Finish##OTHER##,Features##OTHER##,ExpectedLife##OTHER##,DurationUnit##OTHER##,DocumentationTechnical##OTHER##,DocumentationLiterature##OTHER##,DocumentationInstallationGuide##OTHER##,DocumentationCertificates##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Cut Length of Pipe Cover Kit##LENGTH##MILLIMETERS,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Connectors Offset##LENGTH##MILLIMETERS,Connector Z Offset##LENGTH##MILLIMETERS,Connector Y Offset##LENGTH##MILLIMETERS,Color##OTHER##,Cold Water Radius##LENGTH##MILLIMETERS,Cold Water Connection Diameter##LENGTH##MILLIMETERS,CodePerformance##OTHER##,ClassificationValue##OTHER##,ClassificationName##OTHER##,CW Connection Size##LENGTH##MILLIMETERS,CW Connection##OTHER##,BarCode##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Assembly Code##OTHER##,Applications##OTHER##,Accessories##OTHER##,AccessibilityPerformance##OTHER##,A##LENGTH##MILLIMETERS
T113A,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T113A,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A113A

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control, temperature adjustment and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference TSV1-A113A as per drawing No. D10345. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T113A,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T113A,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,1,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A113A/,"Horne Shower Panel with temperature control, timed flow control and vandal resistant head. Supplies from above.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T113B,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,2,T113B,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A113AB

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control, temperature adjustment and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A113AB as per drawing D10345. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T113B,2016,88.999999999998,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T113B,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,1,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A113AB/,"Horne Shower Panel with temperature control, timed flow control and vandal resistant head. Supplies from behind.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T113LR,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,3,T113LR,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE LIGATURE RESISTANT SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A113ALR

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with ligature resistant push button timed flow control, temperature adjustment and vandal and ligature resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference TSV1-A113ALR as per drawing number D11301. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T113LR,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T113LR,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,0,0,1,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-LIGATURE-RESISTANT-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A113ALR/,"Horne Ligature Resistant shower panel with temperature control, timed flow control and vandal resistant shower head. Supplies from above.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T113ALR,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,4,T113ALR,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE LIGATURE RESISTANT SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A113ABLR

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with ligature resistant push button timed flow control, temperature adjustment and ligature and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A113ABLR  as per drawing number D11302. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T113ALR,2016,88.999999999998,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T113ALR,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,0,0,1,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-LIGATURE-RESISTANT-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A113ABLR/,"Horne Ligature Resistant shower panel with temperature control, timed flow control and vandal resistant shower head. Supplies from behind.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T206A,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,5,T206A,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND SWIVEL SHOWER HEAD
TSV1-A206A

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control, temperature adjustment and swivel shower head in chromium plated finish. Product Reference TSV1-A206A as per drawing No. D10347. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T206A,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T206A,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,1,1,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-SWIVEL-SHOWER-HEAD/TSV1-A206A/,"Horne Shower Panel with temperature control, timed flow control and swivel shower head. Supplies from above.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T206B,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,6,T206B,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND SWIVEL SHOWER HEAD
TSV1-A206AB

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control, temperature adjustment and swivel shower head in chromium plated finish. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A206AB as per drawing D10362. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T206B,2016,88.999999999998,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T206B,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,1,1,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-SWIVEL-SHOWER-HEAD/TSV1-A206AB/,"Horne Shower Panel with temperature control, timed flow control and swivel shower head. Supplies from behind.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T113T4,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T113T4,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A113A

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control, temperature adjustment and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference TSV1-A113A as per drawing No. D10345. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T113T4,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T113T4,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,480.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,1,1,0,0,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A113A/,"Horne Shower Panel with temperature control, timed flow control and vandal resistant head. Supplies from above.",1350.000000000000,465.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T113T9,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T113T9,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A113A

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control, temperature adjustment and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference TSV1-A113A as per drawing No. D10345. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T113T9,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T113T9,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,1,1,0,0,1,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A113A/,"Horne Shower Panel with temperature control, timed flow control and vandal resistant head. Supplies from above.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T206T4,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,5,T206T4,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND SWIVEL SHOWER HEAD
TSV1-A206A

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control, temperature adjustment and swivel shower head in chromium plated finish. Product Reference TSV1-A206A as per drawing No. D10347. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T206T4,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T206T4,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,480.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,1,1,1,0,0,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-SWIVEL-SHOWER-HEAD/TSV1-A206A/,"Horne Shower Panel with temperature control, timed flow control and swivel shower head. Supplies from above.",1350.000000000000,465.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T206T9,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,5,T206T9,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. TSV1-3 valve approved under the WRAS scheme, certificate 1111002.","HORNE SHOWER PANEL WITH TEMPERATURE CONTROL, TIMED FLOW CONTROL AND SWIVEL SHOWER HEAD
TSV1-A206A

Includes integral thermostatic shower valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control, temperature adjustment and swivel shower head in chromium plated finish. Product Reference TSV1-A206A as per drawing No. D10347. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne TSV1 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T206T9,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T206T9,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,1,1,1,0,0,1,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/TSV1-A20XA-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TEMPERATURE-CONTROL-TIMED-FLOW-CONTROL-AND-SWIVEL-SHOWER-HEAD/TSV1-A206A/,"Horne Shower Panel with temperature control, timed flow control and swivel shower head. Supplies from above.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,n/a,Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. TSV1 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
