,_distributed by##OTHER##,_current revision##OTHER##,_created by##OTHER##,_authorized by##OTHER##,_BIMspec_GUID##OTHER##,Width##LENGTH##MILLIMETERS,Waste Connection##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabor##OTHER##,WarrantyDescription##OTHER##,Void Height Offset##LENGTH##MILLIMETERS,Void Depth Offset##LENGTH##MILLIMETERS,Vent Connection##OTHER##,URL##OTHER##,TypeName##OTHER##,Type Version##OTHER##,Type Comments##OTHER##,Top Entry Inlets##OTHER##,TagNumber##OTHER##,Sustainability##OTHER##,Standards and Approvals##OTHER##,Specification Clause##OTHER##,SpareParts##OTHER##,Size##OTHER##,Show Pipe Cover##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,ReplacementCost##OTHER##,ReferencedStandard##OTHER##,Rear Entry Inlets##OTHER##,Quick Code##OTHER##,ProductionYear##OTHER##,PipeConnectionOffset##LENGTH##MILLIMETERS,Pipe Cover Warning##OTHER##,Panel & Pipe Cover Material##OTHER##,Operating Conditions##OTHER##,NBSReference##OTHER##,NBSObjectName##OTHER##,NBSNote##OTHER##,NBSDescription##OTHER##,ModelNumber##OTHER##,Mechanical Specification##OTHER##,Maximum Static Pressure##OTHER##,Material##OTHER##,Maintained Water Pressure##OTHER##,Integral Flow Rate##OTHER##,InstallationDate##OTHER##,ILTDU##OTHER##,Hot Water Radius##LENGTH##MILLIMETERS,Height To Ceiling##LENGTH##MILLIMETERS,Model##OTHER##,Manufacturer##OTHER##,Length of Head Pipe##LENGTH##MILLIMETERS,Length##LENGTH##MILLIMETERS,Keynote##OTHER##,Hot Water Connection Diameter##LENGTH##MILLIMETERS,Has Vandal Resistant Shower Head##OTHER##,Has Swivel Shower Head##OTHER##,Has Standard Timed Flow Control##OTHER##,Has Pipe Cover##OTHER##,Has Ligature Resistant Timed Flow Control##OTHER##,Has Key - 6263##OTHER##,Has Flexible Hose and Slide Bar##OTHER##,Has 940mm Pipe Cover Kit##OTHER##,Has 465mm Pipe Cover Kit##OTHER##,HW Connection Size##LENGTH##MILLIMETERS,HW Connection##OTHER##,Grade##OTHER##,Finish##OTHER##,Features##OTHER##,ExpectedLife##OTHER##,DurationUnit##OTHER##,DocumentationTechnical##OTHER##,DocumentationLiterature##OTHER##,DocumentationInstallationGuide##OTHER##,DocumentationCertificates##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Cut Length of Pipe Cover Kit##LENGTH##MILLIMETERS,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Connectors Offset##LENGTH##MILLIMETERS,Connector Z Offset##LENGTH##MILLIMETERS,Connector Y Offset##LENGTH##MILLIMETERS,Color##OTHER##,Cold Water Radius##LENGTH##MILLIMETERS,Cold Water Connection Diameter##LENGTH##MILLIMETERS,CodePerformance##OTHER##,ClassificationValue##OTHER##,ClassificationName##OTHER##,CW Connection Size##LENGTH##MILLIMETERS,CW Connection##OTHER##,BarCode##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Assembly Code##OTHER##,Applications##OTHER##,Accessories##OTHER##,AccessibilityPerformance##OTHER##,A##LENGTH##MILLIMETERS
T109A,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T109A,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A109A

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference TSV1-A109A as per drawing No. D10351. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T109A,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T109A,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,1,0,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A109A/,Horne Shower Panel with timed flow control and vandal resistant shower head. Supplies from above.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T109B,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,2,T109B,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A109AB

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A109AB as per drawing D10358. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T109B,2016,88.999999999998,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T109B,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,1,0,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A109AB/,Horne Shower Panel with timed flow control and vandal resistant shower head. Supplies from behind.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T109ALR,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,3,T109ALR,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH LIGATURE RESISTANT TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A109ALR

Includes integral TMV3 Scheme Approved Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control with ligature resistant bezel and vandal and ligature resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference TSV1-A109ALR as per drawing No. D10352. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T109ALR,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T109ALR,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,0,0,1,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-LIGATURE-RESISTANT-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A109ALR/,Horne Shower Panel with ligature resistant timed flow control and vandal resistant head. Supplies from above.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision in new build, refurbishment, retrofit and temporary installations in secure settings where safety and water economy are key issues.",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T109BLR,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,4,T109BLR,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH LIGATURE RESISTANT TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A109ABLR

Includes integral TMV3 Scheme Approved Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control with ligature resistant shroud and vandal and ligature resistant, adjustable and flow regulated shower head in chromium plated finish. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A109ABLR as per drawing D10349. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T109BLR,2016,88.999999999998,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T109BLR,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,0,0,1,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-LIGATURE-RESISTANT-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A109ABLR/,Horne Shower Panel with ligature resistant timed flow control and vandal resistant head. Supplies from behind.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision in new build, refurbishment, retrofit and temporary installations in secure settings where safety and water economy are key issues",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T306A,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,5,T306A,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND SWIVEL SHOWER HEAD
TSV1-A306A

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and swivel shower head in chromium plated finish. Product Reference TSV1-A306A as per drawing No. D10354. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T306A,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T306A,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,1,0,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-SWIVEL-SHOWER-HEAD/TSV1-A306A/,Horne Shower Panel with timed flow control and swivel shower head. Supplies from above.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T306B,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,6,T306B,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND SWIVEL SHOWER HEAD
TSV1-A306AB

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and swivel shower head in chromium plated finish. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A306AB as per drawing D10357. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T306B,2016,88.999999999998,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T306B,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,1,0,0,0,0,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-SWIVEL-SHOWER-HEAD/TSV1-A306AB/,Horne Shower Panel with timed flow control and swivel shower head. Supplies from behind.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T307A,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,7,T307A,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE TSV1 SHOWER PANEL WITH TIMED FLOW CONTROL, FLEXIBLE HOSE AND SLIDE BAR
TSV1-A307A

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and shower kit, comprising chromium plated three function easy clean shower hand set with flexible hose and slide bar. Product Reference TSV1-A307A as per drawing No. D10355. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T307A,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T307A,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,0,1,0,0,0,1,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-FLEXIBLE-HOSE-AND-SLIDE-BAR/TSV1-A307A/,"Horne TSV1 Shower panel with timed flow control, flexible hose and slide bar. Supplies from above.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T307B,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,200.000000000000,0,www.horne.co.uk,n/a,8,T307B,0,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE TSV1 SHOWER PANEL WITH TIMED FLOW CONTROL, FLEXIBLE HOSE AND SLIDE BAR
TSV1-A307AB

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and shower kit, comprising chromium plated three function easy clean shower hand set with flexible hose and slide bar. Connections by SOFT-PEX flexible braided hose for concealed water supply. Product Reference TSV1-A307AB as per drawing D10379. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,0,Rectangular,Please complete on commissioning,n/a,BS7942:2000,1,T307B,2016,88.999999999998,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T307B,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,0,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,0,1,0,0,0,1,0,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-FLEXIBLE-HOSE-AND-SLIDE-BAR/TSV1-A307AB/,"Horne TSV1 Shower panel with timed flow control, flexible hose and slide bar. Supplies from behind.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,50.000000000000,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T109T4,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T109T4,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A109A

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference TSV1-A109A as per drawing No. D10351. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T109T4,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T109T4,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,480.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,1,1,0,0,0,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A109A/,Horne Shower Panel with timed flow control and vandal resistant shower head. Supplies from above.,1350.000000000000,465.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T109T9,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,1,T109T9,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD
TSV1-A109A

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference TSV1-A109A as per drawing No. D10351. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T109T9,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T109T9,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,1,1,0,0,0,1,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD/TSV1-A109A/,Horne Shower Panel with timed flow control and vandal resistant shower head. Supplies from above.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T306T4,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,5,T306T4,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND SWIVEL SHOWER HEAD
TSV1-A306A

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and swivel shower head in chromium plated finish. Product Reference TSV1-A306A as per drawing No. D10354. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T306T4,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T306T4,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,480.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,1,1,0,0,0,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-SWIVEL-SHOWER-HEAD/TSV1-A306A/,Horne Shower Panel with timed flow control and swivel shower head. Supplies from above.,1350.000000000000,465.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T306T9,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,5,T306T9,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND SWIVEL SHOWER HEAD
TSV1-A306A

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and swivel shower head in chromium plated finish. Product Reference TSV1-A306A as per drawing No. D10354. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T306T9,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T306T9,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,1,1,0,0,0,1,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-SWIVEL-SHOWER-HEAD/TSV1-A306A/,Horne Shower Panel with timed flow control and swivel shower head. Supplies from above.,1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.",Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.,n/a,280.000000000000
T307T4,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,7,T307T4,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE TSV1 SHOWER PANEL WITH TIMED FLOW CONTROL, FLEXIBLE HOSE AND SLIDE BAR
TSV1-A307A

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and shower kit, comprising chromium plated three function easy clean shower hand set with flexible hose and slide bar. Product Reference TSV1-A307A as per drawing No. D10355. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T307T4,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T307T4,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,480.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,0,1,1,0,0,1,0,1,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-FLEXIBLE-HOSE-AND-SLIDE-BAR/TSV1-A307A/,"Horne TSV1 Shower panel with timed flow control, flexible hose and slide bar. Supplies from above.",1350.000000000000,465.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
T307T9,www.bimstore.co.uk,2,Ian Holmes,Kris Atkinson,0,180.000000000000,0,Please complete on commissioning,Horne Engineering Ltd,n/a,Years,2,n/a,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,150.000000000000,0.000000000000,0,www.horne.co.uk,n/a,7,T307T9,1,n/a,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating. Alternative flow regulators available upon request.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224. H1503 thermostatic mixing valve WRAS approved - certificate number 1209103.","HORNE TSV1 SHOWER PANEL WITH TIMED FLOW CONTROL, FLEXIBLE HOSE AND SLIDE BAR
TSV1-A307A

Includes integral Horne 15 H1503 thermostatic mixing valve pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and shower kit, comprising chromium plated three function easy clean shower hand set with flexible hose and slide bar. Product Reference TSV1-A307A as per drawing No. D10355. To be installed according to the manufacturer's instructions and commissioned in accordance with water regulations and bylaws using the Horne 15 Flushing kit.",n/a,H: 1015mm W: 181mm D: 215mm,1,Rectangular,Please complete on commissioning,n/a,BS7942:2000,0,T307T9,2016,89.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,"Range of maintained water supply pressures 0.5 - 3 bar, range of hot water supply temperatures  52 - 85 deg C, max differential between hot water temperature and mixed water temperature 5 deg C, hot and cold water supply pressures do not need to be equal, however, the lower of the supply pressures should not be less than 0.2 bar.",45-35-70/330,Shower fittings package,,Shower fittings package,T307T9,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,Please complete on commissioning,1,7.500000000000,955.000000000000,TSV1 Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,0,1,1,0,0,1,1,0,15.000000000000,1,n/a,Powder Coated,n/a,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/H15-TFC-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-TSV1-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-FLEXIBLE-HOSE-AND-SLIDE-BAR/TSV1-A307A/,"Horne TSV1 Shower panel with timed flow control, flexible hose and slide bar. Supplies from above.",1350.000000000000,940.000000000000,April 2016,sales@horne.co.uk,n/a,25.500000000000,15.000000000000,565.000000000000,White RAL 9010,7.500000000000,15.000000000000,"Designed to meet requirements of BS7942:2000, approved under the TMV3 Scheme to NHS Model Engineering Specifications D 08, WRAS Approved",Pr_40_20_87_75,Uniclass2015,15.000000000000,1,Please complete on commissioning,Fixed,Please complete on commissioning,D2010700,"Shower provision for new build, refurbishment, retrofit and temporary installations in sport and leisure settings or where water conservation is a key requirement.","2 meter Hose, Pipe cover - SA-465PC OR SA-940PC. H15 Flushing Kit. Monitoring Kit.",n/a,280.000000000000
