,_distributed by##OTHER##,_current revision##OTHER##,_created by##OTHER##,_author##OTHER##,_BIMspec_GUID##OTHER##,Width##LENGTH##MILLIMETERS,Waste Connection##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyGuarantorLabor##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDurationLabour##OTHER##,WarrantyDescription##OTHER##,Version##OTHER##,Vent Connection##OTHER##,Uniclass2##OTHER##,URL##OTHER##,Type Version##OTHER##,Type Comments##OTHER##,Top Entry Inlets##OTHER##,Sustainability##OTHER##,Standards and Approvals##OTHER##,Specification Clause##OTHER##,SpareParts##OTHER##,Size##OTHER##,Show Pipe Cover##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,ReplacementCost##OTHER##,ReferencedStandard##OTHER##,Rear Entry Inlets##OTHER##,Quick Code##OTHER##,ProductionYear##OTHER##,Pre Mixed Connection Size##LENGTH##MILLIMETERS,Pipe Cover Warning##OTHER##,Panel & Pipe Cover Material##OTHER##,Operating Conditions##OTHER##,NBSTypeID##OTHER##,NBSReference##OTHER##,NBSObjectName##OTHER##,NBSNote##OTHER##,ModelNumber##OTHER##,Mechanical Specification##OTHER##,Maximum Static Pressure##OTHER##,Material##OTHER##,Maintained Water Pressure##OTHER##,Integral Flow Rate##OTHER##,InstallationDate##OTHER##,Hot Water Radius##LENGTH##MILLIMETERS,Height To Ceiling##LENGTH##MILLIMETERS,Model##OTHER##,Manufacturer##OTHER##,Length of Head Pipe##LENGTH##MILLIMETERS,Length##LENGTH##MILLIMETERS,Keynote##OTHER##,Hot Water Connection Diameter##LENGTH##MILLIMETERS,Has Vandal Resistant Shower Head##OTHER##,Has Standard Timed Flow Control##OTHER##,Has Pipe Cover##OTHER##,Has Ligature Resistant Timed Flow Control##OTHER##,Has Flexible Hose and Slide Bar##OTHER##,Has 940mm Pipe Cover Kit##OTHER##,Has 465mm Pipe Cover Kit##OTHER##,HW Connection Size##LENGTH##MILLIMETERS,HW Connection##OTHER##,Grade##OTHER##,Finish##OTHER##,Features##OTHER##,ExpectedLife##OTHER##,DurationUnit##OTHER##,DocumentationTechnical##OTHER##,DocumentationLiterature##OTHER##,DocumentationInstallationGuide##OTHER##,DocumentationCertificates##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Cut Length of Pipe Cover Kit##LENGTH##MILLIMETERS,CreatedOn##OTHER##,CreatedBy##OTHER##,Constituents##OTHER##,Connector Z Offset##LENGTH##MILLIMETERS,Connector Y Offset##LENGTH##MILLIMETERS,Color##OTHER##,Cold Water Radius##LENGTH##MILLIMETERS,Cold Water Connection Diameter##LENGTH##MILLIMETERS,CodePerformance##OTHER##,ClassificationValue##OTHER##,ClassificationName##OTHER##,CW Connection Size##LENGTH##MILLIMETERS,CW Connection##OTHER##,BarCode##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,Assembly Code##OTHER##,Applications##OTHER##,Accessories##OTHER##,AccessibilityPerformance##OTHER##,A##LENGTH##MILLIMETERS
SP A110A,www.bimstore.co.uk,1,www.bimstore.co.uk,Andy Smart,0,180.000000000000,0,,Horne Engineering Ltd,,Years,2,0,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,,0,45-35-70/330,www.horne.co.uk,1,SP A110A,1,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD FOR USE WITH PRE-BLENDED WATER SUPPLY ONLY
SP-A110A

Pre-plumbed white, polyester powder coated aluminium panel including push button timed flow control and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference SP-A110A as per drawing No. D10350.  For use with pre-blended water supply only and to be installed according to the manufacturer's instructions.",,H: 1015mm W: 181mm D: 215mm,0,Rectangular,,,BS7942:2000,0,SP A110A,2014,15.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,Range of maintained mixed water supply pressures 0.5 - 3.0 bar.,,,,,SP A110A,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,,7.500000000000,955.000000000000,SP Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,0,0,0,0,15.000000000000,1,,Powder Coated,,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Group-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD-FOR-USE-WITH-PRE-BLENDED-WATER-SUPPLY-ONLY/SP-A110A/,Horne Shower Panel with timed flow control and vandal resistant shower head for use with pre-blended water supply only,1350.000000000000,940.000000000000,September 2014,sales@horne.co.uk,,0.000000000000,592.500000000000,White RAL 9010,7.500000000000,15.000000000000,N/A,L7214,Uniclass1.4,15.000000000000,1,,Fixed,,D2010700,"Group shower (pre-mixed water supply) provision for new build, refurbishment, retrofit and temporary installations where water conservation is a key requirement",Pipe cover - SA-465PC OR SA-940PC,N/A,280.000000000000
SP A407AB,www.bimstore.co.uk,1,www.bimstore.co.uk,Andy Smart,0,180.000000000000,0,,Horne Engineering Ltd,,Years,2,0,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,,0,45-35-70/330,www.horne.co.uk,6,SP A407AB,0,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL, FLEXIBLE HOSE AND SLIDE BAR (For use with pre-blended water supply only)
SP-A407AB

pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and shower kit comprising chromium plated three function easy clean and flow regulated shower hand set with flexible hose and slide bar. Mixed water connection by SOFT-PEX flexible braided hose for concealed supply.  Product Reference SP-A407AB as per drawing D10360. For use with pre-blended water supply only and to be installed according to the manufacturer's instructions.",,H: 1015mm W: 181mm D: 215mm,0,Rectangular,,,BS7942:2000,1,SP A407AB,2014,15.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,Range of maintained mixed water supply pressures 0.5 - 3.0 bar.,,,,,SP A407AB,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,,7.500000000000,955.000000000000,SP Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,0,0,1,0,0,15.000000000000,1,,Powder Coated,,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Group-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-FLEXIBLE-HOSE-AND-SLIDE-BAR-PUSH-BUTTON-TIMED-FLOW-CONTROL/SP-A407AB/,"Horne Shower Panel with timed flow control, flexible hose and slide bar (for use with pre-blended water supply only)",1350.000000000000,940.000000000000,September 2014,sales@horne.co.uk,,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,N/A,L7214,Uniclass1.4,15.000000000000,1,,Fixed,,D2010700,"Group shower (pre-mixed water supply) provision for new build, refurbishment, retrofit and temporary installations where water conservation is a key requirement",Pipe cover - SA-465PC OR SA-940PC,N/A,280.000000000000
SP A110ABLR,www.bimstore.co.uk,1,www.bimstore.co.uk,Andy Smart,0,180.000000000000,0,,Horne Engineering Ltd,,Years,2,0,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,,0,45-35-70/330,www.horne.co.uk,4,SP A110ABLR,0,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224.","HORNE LIGATURE RESISTANT SHOWER PANEL WITH TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD FOR USE WITH PRE-BLENDED WATER SUPPLY ONLY
SP-A110ABLR

Pre-plumbed white, polyester powder coated aluminium panel with ligature resistant fittings including push button timed flow control and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Connections by SOFT-PEX flexible braided hose for concealed water supply.  Product Reference SP-A110ABLR as per drawing No. D11304. For use with pre-blended water supply only and to be installed according to the manufacturer's instructions.",,H: 1015mm W: 181mm D: 215mm,0,Rectangular,,,BS7942:2000,1,SP A110ABLR,2014,15.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,Range of maintained mixed water supply pressures 0.5 - 3.0 bar.,,,,,SP A110ABLR,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,,7.500000000000,955.000000000000,SP Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,0,1,0,0,0,15.000000000000,1,,Powder Coated,,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Group-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-LIGATURE-RESISTANT-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD-FOR-USE-WITH-PRE-BLENDED-WATER-SUPPLY-ONLY/SP-A110ABLR/,Horne Ligature Resistant Shower Panel with timed flow control and vandal resistant shower head for use with pre-blended water supply only,1350.000000000000,940.000000000000,September 2014,sales@horne.co.uk,,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,N/A,L7214,Uniclass1.4,15.000000000000,1,,Fixed,,D2010700,"Group shower (pre-mixed water supply) provision for new build, refurbishment, retrofit and temporary installations where water conservation is a key requirement",Pipe cover - SA-465PC OR SA-940PC,N/A,280.000000000000
SP A110ALR,www.bimstore.co.uk,1,www.bimstore.co.uk,Andy Smart,0,180.000000000000,0,,Horne Engineering Ltd,,Years,2,0,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,,0,45-35-70/330,www.horne.co.uk,3,SP A110ALR,1,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224.","HORNE LIGATURE RESISTANT SHOWER PANEL WITH TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD FOR USE WITH PRE-BLENDED WATER SUPPLY ONLY
SP-A110ALR

Pre-plumbed white, polyester powder coated aluminium panel with ligature resistant fittings including push button timed flow control and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Product Reference SP-A110ALR as per drawing No. D11303.  For use with pre-blended water supply only and to be installed according to the manufacturer's instructions.",,H: 1015mm W: 181mm D: 215mm,0,Rectangular,,,BS7942:2000,0,SP A110ALR,2014,15.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,Range of maintained mixed water supply pressures 0.5 - 3.0 bar.,,,,,SP A110ALR,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,,7.500000000000,955.000000000000,SP Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,0,0,1,0,0,0,15.000000000000,1,,Powder Coated,,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Group-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-LIGATURE-RESISTANT-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD-FOR-USE-WITH-PRE-BLENDED-WATER-SUPPLY-ONLY/SP-A110ALR/,Horne Ligature Resistant Shower Panel with timed flow control and vandal resistant shower head for use with pre-blended water supply only,1350.000000000000,940.000000000000,September 2014,sales@horne.co.uk,,0.000000000000,592.500000000000,White RAL 9010,7.500000000000,15.000000000000,N/A,L7214,Uniclass1.4,15.000000000000,1,,Fixed,,D2010700,"Group shower (pre-mixed water supply) provision for new build, refurbishment, retrofit and temporary installations where water conservation is a key requirement",Pipe cover - SA-465PC OR SA-940PC,N/A,280.000000000000
SP A110AB,www.bimstore.co.uk,1,www.bimstore.co.uk,Andy Smart,0,180.000000000000,0,,Horne Engineering Ltd,,Years,2,0,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,,0,45-35-70/330,www.horne.co.uk,2,SP A110AB,0,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL AND VANDAL RESISTANT SHOWER HEAD FOR USE WITH PRE-BLENDED WATER SUPPLY ONLY
SP-A110AB

Pre-plumbed white, polyester powder coated aluminium panel including push button timed flow control and vandal resistant, adjustable and flow regulated shower head in chromium plated finish. Mixed water connection by SOFT-PEX flexible braided hose for concealed water supply. Product Reference SP-A110AB as per drawing D10359. For use with pre-blended water supply only and to be installed according to the manufacturer's instructions.",,H: 1015mm W: 181mm D: 215mm,0,Rectangular,,,BS7942:2000,1,SP A110AB,2014,15.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,Range of maintained mixed water supply pressures 0.5 - 3.0 bar.,,,,,SP A110AB,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,,7.500000000000,955.000000000000,SP Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,1,1,0,0,0,0,0,15.000000000000,1,,Powder Coated,,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Group-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-TIMED-FLOW-CONTROL-AND-VANDAL-RESISTANT-SHOWER-HEAD-FOR-USE-WITH-PRE-BLENDED-WATER-SUPPLY-ONLY/SP-A110AB/,Horne Shower Panel with timed flow control and vandal resistant shower head for use with pre-blended water supply only,1350.000000000000,940.000000000000,September 2014,sales@horne.co.uk,,109.000000000000,468.300000000000,White RAL 9010,7.500000000000,15.000000000000,N/A,L7214,Uniclass1.4,15.000000000000,1,,Fixed,,D2010700,"Group shower (pre-mixed water supply) provision for new build, refurbishment, retrofit and temporary installations where water conservation is a key requirement",Pipe cover - SA-465PC OR SA-940PC,N/A,280.000000000000
SP A407A,www.bimstore.co.uk,1,www.bimstore.co.uk,Andy Smart,0,180.000000000000,0,,Horne Engineering Ltd,,Years,2,0,Horne Engineering Ltd guarantee their products against any defect in materials or workmanship for 2 years from the date of purchase.,,0,45-35-70/330,www.horne.co.uk,5,SP A407A,1,Integral flow regulator (8 L/min) for water and energy conservation and contributes to BREEAM rating.,"BS7942:2000, 'Thermostatic mixing valves for use in care establishments' and is approved, under the TMV3 Scheme, to NHS Model Engineering Specifications D 08 Thermostatic mixing valves (Healthcare premises). WRAS approved product. Manufactured to BS EN ISO 9001:2000. Certificate No. FM1224.","HORNE SHOWER PANEL WITH TIMED FLOW CONTROL, FLEXIBLE HOSE AND SLIDE BAR (For use with pre-blended water supply only)
SP-A407A

pre-plumbed within a white polyester powder coated aluminium panel with push button timed flow control and shower kit comprising chromium plated three function easy clean and flow regulated shower hand set with flexible hose and slide bar. Product Reference SP-A407A as per drawing No. D10356.  For use with pre-blended water supply only and to be installed according to the manufacturer's instructions.",,H: 1015mm W: 181mm D: 215mm,0,Rectangular,,,BS7942:2000,0,SP A407A,2014,15.000000000000,OK,Horne Engineering - Powder Coated Aluminium - White RAL 9010,Range of maintained mixed water supply pressures 0.5 - 3.0 bar.,,,,,SP A407A,"Connection to mixed water supply by compression fitting to suit 15mm copper pipe, working parts protected from water borne debris by 250 micron fine mesh strainer, integral check valves in hot and cold supplies included, thermostatic mixing valve body in CZ 132 brass , spray plate featuring anti scale silicone rubber membrane with nozzle array. Angle of spray adjustable from 19 - 24 degrees.",10 bar,"Aluminium extrusion, brass valve",0.2 - 5 bar,8 L/min,,7.500000000000,955.000000000000,SP Shower Panel,Horne Engineering Ltd,85.000000000000,1015.000000000000,N13/230,15.000000000000,0,1,0,0,1,0,0,15.000000000000,1,,Powder Coated,,0,Years,http://www.horne.co.uk/Resources/Horne-Literature/PRODUCT-INSTRUCTIONS/Group-Shower-Panel-Instructions/,http://www.horne.co.uk/Resources/Horne-Literature/Shower-Panel-Specification-Manual/,http://www.horne.co.uk/Products/Shower-Panels/Shower-Panel-Installation-and-Maintenance/,http://www.horne.co.uk/HORNE-SHOWER-PANEL-WITH-FLEXIBLE-HOSE-AND-SLIDE-BAR-PUSH-BUTTON-TIMED-FLOW-CONTROL/SP-A407A/,"Horne Shower Panel with timed flow control, flexible hose and slide bar (for use with pre-blended water supply only)",1350.000000000000,940.000000000000,September 2014,sales@horne.co.uk,,0.000000000000,592.500000000000,White RAL 9010,7.500000000000,15.000000000000,N/A,L7214,Uniclass1.4,15.000000000000,1,,Fixed,,D2010700,"Group shower (pre-mixed water supply) provision for new build, refurbishment, retrofit and temporary installations where water conservation is a key requirement",Pipe cover - SA-465PC OR SA-940PC,N/A,280.000000000000
