,Form##OTHER##,IntegralAccessories##OTHER##,BIMObjectName##OTHER##,NBSVariantId##OTHER##,HasStandardControls##OTHER##,HasLigatureResistantControls##OTHER##,HasLeverControls##OTHER##,PipeCoverHeight##LENGTH##MILLIMETERS,ModelNumber##OTHER##,Name##OTHER##,NominalHeight##LENGTH##MILLIMETERS,Size##OTHER##
StandardControls940mmPipeCoverT105T9,"Wall-mounted shower panel with thermostatic mixer valve, hand controls, vandal resistant shower head, ILTDU and pipe cover",Integral in-line thermal disinfection unit and 940 mm pipe cover,NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_StandardControls940mmPipeCoverT105T9,1918889f-22dd-4b57-a4ad-4f1f202054eb,1,0,0,930,T105T9,ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_StandardControls940mmPipeCoverT105T9_HorneEngineeringLtd,1968,180 x 128 x 1968 mm
StandardControls465mmPipeCoverT105T4,"Wall-mounted shower panel with thermostatic mixer valve, hand controls, vandal resistant shower head, ILTDU and pipe cover",Integral in-line thermal disinfection unit and 465 mm pipe cover,NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_StandardControls465mmPipeCoverT105T4,6f649e14-eb8a-44be-8e35-c4dcd7c20431,1,0,0,455,T105T4,ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_StandardControls465mmPipeCoverT105T4_HorneEngineeringLtd,1493,180 x 128 x 1493 mm
LeverControls940mmPipeCoverT105T92L,"Wall-mounted shower panel with thermostatic mixer valve, lever controls, vandal resistant shower head, ILTDU and pipe cover",Integral in-line thermal disinfection unit and 940 mm pipe cover,NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_LeverControls940mmPipeCoverT105T92L,e8ba44c1-fc14-42c5-b2f3-b20b48306657,0,0,1,930,T105T92L,ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_LeverControls940mmPipeCoverT105T92L_HorneEngineeringLtd,1968,180 x 128 x 1968 mm
LigatureResistantControls940mmPipeCoverT105T9LR,"Wall-mounted shower panel with thermostatic mixer valve, ligature resistant hand controls, vandal and ligature resistant shower head, ILTDU and pipe cover",Integral in-line thermal disinfection unit and 940 mm pipe cover,NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_LigatureResistantControls940mmPipeCoverT105T9LR,31c4a478-ec0a-487c-82f1-a3da27b77bdb,0,1,0,930,T105T9LR,ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_LigatureResistantControls940mmPipeCoverT105T9LR_HorneEngineeringLtd,1968,180 x 128 x 1968 mm
LigatureResistantControls465mmPipeCoverT105T4LR,"Wall-mounted shower panel with thermostatic mixer valve, ligature resistant hand controls, vandal and ligature resistant shower head, ILTDU and pipe cover",Integral in-line thermal disinfection unit and 465 mm pipe cover,NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_LigatureResistantControls465mmPipeCoverT105T4LR,b268a2c6-4e34-4f55-aee5-3713f21a9369,0,0,0,455,T105T4LR,ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_LigatureResistantControls465mmPipeCoverT105T4LR_HorneEngineeringLtd,1493,180 x 128 x 1493 mm
LeverControls465mmPipeCoverT105T42L,"Wall-mounted shower panel with thermostatic mixer valve, lever controls, vandal resistant shower head, ILTDU and pipe cover",Integral in-line thermal disinfection unit and 465 mm pipe cover,NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_LeverControls465mmPipeCoverT105T42L,72e61ef8-8bff-4307-b289-c1d5c7b76a5b,0,0,1,455,T105T42L,ShowerFittingsPackage_PanelShowerWithDualControlsVandalAndLigatureResistantHeadInclILTDU_LeverControls465mmPipeCoverT105T42L_HorneEngineeringLtd,1493,180 x 128 x 1493 mm
