,Accessories##OTHER##,Form##OTHER##,MaterialsFinishAndColour##OTHER##,BIMObjectName##OTHER##,NBSVariantId##OTHER##,HasStandardControls##OTHER##,HasLeverControls##OTHER##,RailMaterial##OTHER##,HasRearEntryInlets##OTHER##,CodePerformance##OTHER##,ModelNumber##OTHER##,Name##OTHER##
TopEntryInletsStandardControlsWhiteRiserRailT107A,"Flushing kit, P/N 5138,465 mm Pipe cover kit, P/N SA-465PC,940 mm Pipe cover kit, P/N SA-940PC,2 metre hose, P/N SA-108B,Wall-mounted grab rail, white/grey, P/N 70-6011,Wall-mounted grab rail, orange/grey, P/N 70-6012","Wall-mounted shower panel with thermostatic mixer valve, dual hand controls, three function handset, hose and riser rail","Epoxy-polyester powder-coated white (RAL 9010) panel, chromium-plated shower head and hand controls, white riser rail",NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_TopEntryInletsStandardControlsWhiteRiserRailT107A,978d26a9-3291-41b0-83d4-c192f3109265,1,0,NBS_HorneEngineeringLtd_White,0,Type 3 and UK Water Regulation 4 Approved (previously TMV3 Scheme and WRAS Approval respectively),T107A,ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_TopEntryInletsStandardControlsWhiteRiserRailT107A_HorneEngineeringLtd
TopEntryInletsLeverControlsOrangeRiserRailT1Y7A2L,"Flushing kit, P/N 5138,465 mm Pipe cover kit, P/N SA-465PC,940 mm Pipe cover kit, P/N SA-940PC,2 metre hose, P/N SA-108B,Wall-mounted grab rail, orange/grey, P/N 70-6012,Wall-mounted grab rail, white/grey, P/N 70-6011","Wall-mounted shower panel with thermostatic mixer valve, lever controls, three function handset, hose and riser rail","Epoxy-polyester powder-coated white (RAL 9010) panel, chromium-plated shower head and hand controls, orange riser rail",NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_TopEntryInletsLeverControlsOrangeRiserRailT1Y7A2L,55289bcb-4db0-d6be-6b87-69e200fcf77d,0,1,NBS_HorneEngineeringLtd_DeepOrange,0,"Type 3 and UK Water Regulation 4 Approved (equivalent to  TMV3 and WRAS approved), BS 8300",T1Y7A2L,ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_TopEntryInletsLeverControlsOrangeRiserRailT1Y7A2L_HorneEngineeringLtd
RearEntryInletsStandardControlsOrangeRiserRailT1Y7B,"Flushing kit, P/N 5138,2 metre hose, P/N SA-108B,Wall-mounted grab rail, orange/grey, P/N 70-6012,Wall-mounted grab rail, white/grey, P/N 70-6011","Wall-mounted shower panel with thermostatic mixer valve, dual hand controls, three function handset, hose, riser rail and Soft-PEX braided hose connections","Epoxy-polyester powder-coated white (RAL 9010) panel, chromium-plated shower head and hand controls, orange riser rail",NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_RearEntryInletsStandardControlsOrangeRiserRailT1Y7B,dae7de32-5929-5c93-f854-876fb5dda4f5,1,0,NBS_HorneEngineeringLtd_DeepOrange,1,Type 3 and UK Water Regulation 4 Approved (equivalent to  TMV3 and WRAS approved),T1Y7B,ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_RearEntryInletsStandardControlsOrangeRiserRailT1Y7B_HorneEngineeringLtd
TopEntryInletsLeverControlsWhiteRiserRailT107A2L,"Flushing kit, P/N 5138,465 mm Pipe cover kit, P/N SA-465PC,940 mm Pipe cover kit, P/N SA-940PC,2 metre hose, P/N SA-108B,Wall-mounted grab rail, white/grey, P/N 70-6011,Wall-mounted grab rail, orange/grey, P/N 70-6012","Wall-mounted shower panel with thermostatic mixer valve, lever controls, three function handset, hose and riser rail","Epoxy-polyester powder-coated white (RAL 9010) panel, chromium-plated shower head and hand controls, white riser rail",NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_TopEntryInletsLeverControlsWhiteRiserRailT107A2L,98e2d8e4-0c36-430f-9a18-aa18b2bc3c60,0,1,NBS_HorneEngineeringLtd_White,0,"Type 3 and UK Water Regulation 4 Approved (equivalent to  TMV3 and WRAS approved), BS 8300",T107A2L,ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_TopEntryInletsLeverControlsWhiteRiserRailT107A2L_HorneEngineeringLtd
RearEntryInletsLeverControlsOrangeRiserRailT1Y7B2L,"Flushing kit, P/N 5138,2 metre hose, P/N SA-108B,Wall-mounted grab rail, orange/grey, P/N 70-6012,Wall-mounted grab rail, white/grey, P/N 70-6011","Wall-mounted shower panel with thermostatic mixer valve, lever controls, three function handset, hose, riser rail and Soft-PEX braided hose connections","Epoxy-polyester powder-coated white (RAL 9010) panel, chromium-plated shower head and hand controls, orange riser rail",NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_RearEntryInletsLeverControlsOrangeRiserRailT1Y7B2L,dad8693d-e3af-7779-0c20-ee17003e123d,0,1,NBS_HorneEngineeringLtd_DeepOrange,1,"Type 3 and UK Water Regulation 4 Approved (equivalent to  TMV3 and WRAS approved), BS 8300",T1Y7B2L,ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_RearEntryInletsLeverControlsOrangeRiserRailT1Y7B2L_HorneEngineeringLtd
TopEntryInletsStandardControlsOrangeRiserRailT1Y7A,"Flushing kit, P/N 5138,465 mm Pipe cover kit, P/N SA-465PC,940 mm Pipe cover kit, P/N SA-940PC,2 metre hose, P/N SA-108B,Wall-mounted grab rail, orange/grey, P/N 70-6012,Wall-mounted grab rail, white/grey, P/N 70-6011","Wall-mounted shower panel with thermostatic mixer valve, dual hand controls, three function handset, hose and riser rail","Epoxy-polyester powder-coated white (RAL 9010) panel, chromium-plated shower head and hand controls, orange riser rail",NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_TopEntryInletsStandardControlsOrangeRiserRailT1Y7A,696a4a68-ff80-d0d1-6ac1-fee66e735f60,1,0,NBS_HorneEngineeringLtd_DeepOrange,0,Type 3 and UK Water Regulation 4 Approved (equivalent to  TMV3 and WRAS approved),T1Y7A,ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_TopEntryInletsStandardControlsOrangeRiserRailT1Y7A_HorneEngineeringLtd
RearEntryInletsStandardControlsWhiteRiserRailT107B,"Flushing kit, P/N 5138,2 metre hose, P/N SA-108B,Wall-mounted grab rail, white/grey, P/N 70-6011,Wall-mounted grab rail, orange/grey, P/N 70-6012","Wall-mounted shower panel with thermostatic mixer valve, dual hand controls, three function handset, hose, riser rail and Soft-PEX braided hose connections","Epoxy-polyester powder-coated white (RAL 9010) panel, chromium-plated shower head and hand controls, white riser rail",NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_RearEntryInletsStandardControlsWhiteRiserRailT107B,e5873e48-865f-4556-a95a-306ece3734ee,1,0,NBS_HorneEngineeringLtd_White,1,Type 3 and UK Water Regulation 4 Approved (equivalent to  TMV3 and WRAS approved),T107B,ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_RearEntryInletsStandardControlsWhiteRiserRailT107B_HorneEngineeringLtd
RearEntryInletsLeverControlsWhiteRiserRailT107B2L,"Flushing kit, P/N 5138,2 metre hose, P/N SA-108B,Wall-mounted grab rail, white/grey, P/N 70-6011,Wall-mounted grab rail, orange/grey, P/N 70-6012","Wall-mounted shower panel with thermostatic mixer valve, lever controls, three function handset, hose, riser rail and Soft-PEX braided hose connections","Epoxy-polyester powder-coated white (RAL 9010) panel, chromium-plated shower head and hand controls, white riser rail",NBS_HorneEngineeringLtd_ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_RearEntryInletsLeverControlsWhiteRiserRailT107B2L,a8b1adf1-e791-1144-84ac-b99999d0674c,0,1,NBS_HorneEngineeringLtd_White,1,"Type 3 and UK Water Regulation 4 Approved (equivalent to  TMV3 and WRAS approved), BS 8300",T107B2L,ShowerFittingsPackage_PanelShowerWithDualControlsRiserHoseAndThreeFunctionHandsetExclILTDU_RearEntryInletsLeverControlsWhiteRiserRailT107B2L_HorneEngineeringLtd
